VisualOn ALAC decoder support format:

|  |  |  |
| --- | --- | --- |
| Channel | Sample rate | Sample bits |
| 1, 2 | 8-48khz | 16, 24 |